Smelecom Dsp3+

|  |
| --- |
| DSP Ⅲ+ is the most complete programming device for digital odometers, airbag modules, car radios, car immobilizers. It is a high-quality embeded system, which offers a maximum of flexibility and working comfort.  10 years warranty (just for machine) |
|  |

**Technical reference**  
Powered by industrial grade core board with Freescale i.MX28x processor, speeds up to 650MHZ, 800\*480 TFT LCD and touch screen(7.0".16:9). Convenient keyset. USB host and USB device. SD card interface. 128MB NandFlash, 128MB DDRII.  
We use industrial grade components to ensure the stability and reliability under a wide temperature range, from -40℃ to +85℃.  
Whole machine passed EMC industry 4 grade quality assurance and durable performance, the product stability greatly improved.  
The Wince6.0 operating system can ensure the software platform reliability and compatibility.  
Self-check function integrated in system.   
Enhanced OBD functions, including CAN-BUS / J1850 / CCD-BUS / ISO9141 / SPI protocols.  
Intuitive operability by full menu and picture guidance. All data can be edited, stored and loaded.   
Color connection picture is on the screen whenever you need.  
The stored data can be transferred to a PC by USB port or SD card, and also can be transfer to wherever you want directly by internet.  
Update directly from internet.