Product Description

Online Version Kess V5.017 with Red PCB Support 140 Protocol No Token Limited

**Kess V2 V5.017 Online Version No Tokens Limitation V2.7 Kess V2 OBD2 Manager Tuning Kit Auto Truck ECU Programmer  
  
Kess 5.017 With NEW K-Suite 2.7 with exactly 7400 Vehicles added.  
Multi-language available:** English, German, Spanish, Italian, Portuguese, French.  
   
**Kess V2 V5.017 Feature:**  
  
1. Online Version Kess V2 Firmware V5.017 support online service by interent connection  
2. 100% No Tokens Need for all vehicles, no tokens reset button, you can use Kess V5.017 for lifetime  
3. Kess V2 Ksuite V2.7 Firmware V5.017 cover all major brands and protocols including Line, KAN, EDC17 and MED17 and for Ford J1850.  
4.  KESS V2 V5.017 can support cars/trucks/tractors/bikes! KESS V2 supports vehicles accroding to engine. So V5.017 KESS V2 can support new vehicles!  
5. Kess V2 V5.017can read and write ECU via OBD2 port directly, no need to disassemble ECU from the car, easy to use.  
   
**Kess V2 V5.017 Online Version other features:**  
  
**Newest software: Ksuite V2.7**  
KESS V5.017 software is very easy to install, just follow the tips to  click "Next Step", then it will work fine!  
  
**Kess V2 Software Display:**  
  
**Kess V2 V5.017 Online Version Advantage in PC board:**  
  
1. The left upper corner and the lower right corner notch size is not the same  
2. More than  buzzer  
3. WFs = Infineon, BCR112 NPN Digital Transistor  
4. 27E = ON Semiconductor NUP2105LT1G  
5. 6DW = NXP BC817,215 NPN Bipolar Transistor  
6. A6c =MMUN2113LT1G / MMUN2113LT3G  
7. K5B = BC807-25-7-F PNP Bipolar Transistor  
8. Using imported Japanese Murata filter NFE61PT472C1H9L